GLOVE COMPARTMENT LIGHT BULB REMOVAL/INSTALLATION

#
GLOVE COMPARTMENT LIGHT BULB REMOVAL/INSTALLATION

B3E091851445W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front scuff plate (Passenger's side) (SeeFRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (2) Front side trim (Passenger's side) (SeeFRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (3) Decoration panel (SeeDECORATION PANEL REMOVAL/INSTALLATION.)
  (4) Glove compartment (SeeGLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Remove the socket, then remove the glove compartment light bulb.

4. Install in the reverse order of removal.