INTRUDER SENSOR REMOVAL/INSTALLATION

#
INTRUDER SENSOR REMOVAL/INSTALLATION

B3E091400172W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Sunroof seaming welt (vehicles with sunroof)
  (2) Console (4SD) (See CONSOLE REMOVAL/INSTALLATION.)
  (3) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (4) Upper anchor of the front seat belt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)
  (5) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (6) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (7) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)
  (8) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)
  (9) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (10) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (11) Trunk side upper trim (5HB) (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION.)
  (12) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)
  (13) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (14) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (15) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (16) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

3. Disconnect the intruder sensor.

4. Remove the screws.

5. Remove the intruder sensor.

6. Install in the reverse order of removal.