DTC TABLE [FN4A-EL]

#
DTC TABLE [FN4A-EL]

B3E050219090W05

DTC No. | Condition | MIL | AT warning light illuminates | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0011 | CMP-timing over-advanced | (See DTC TABLE [ZJ, Z6].)
P0012 | CMP-timing over-retarded | (See DTC TABLE [ZJ, Z6].)
P0031 | Front HO2S heater control circuit low | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0032 | Front HO2S heater control circuit high | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0037 | Rear HO2S heater control circuit low | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0038 | Rear HO2S heater control circuit high | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0101 | MAF sensor circuit range/performance problem | (See DTC TABLE [LF].)
P0102 | MAF sensor circuit low input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0103 | MAF sensor circuit high input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0107 | MAP sensor circuit low input | (See DTC TABLE [LF].)
P0108 | MAP sensor circuit high input | (See DTC TABLE [LF].)
P0111 | IAT sensor circuit range/performance problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0112 | IAT sensor circuit low input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0113 | IAT sensor circuit high input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0117 | ECT sensor circuit low input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0118 | ECT sensor circuit high input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0121 | TP sensor circuit range/performance problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0122 | TP sensor circuit low input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0123 | TP sensor circuit high input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0125 | Insufficient coolant temperature for closed loop fuel control | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0132 | Front HO2S circuit high voltage | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0133 | Front HO2S circuit slow response | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0134 | Front HO2S circuit no activity detected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0138 | Rear HO2S circuit high voltage | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0140 | Rear HO2S circuit no activity detected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0300 | Random misfire detected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0301 | Cylinder No.1 misfire detected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0302 | Cylinder No.2 misfire detected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0303 | Cylinder No.3 misfire detected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0304 | Cylinder No.4 misfire detected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0327 | KS circuit low input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0328 | KS circuit high input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0335 | CKP sensor circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0340 | CMP sensor circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0403 | EGR control circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0420 | Catalyst system efficiency below threshold | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0443 | Purge solenoid valve circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0480 | Cooling fan control circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0500 | VSS circuit malfunction (MTX) | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
VSS circuit malfunction (ATX) | ON | YES | 2 | CCM | X | (See DTC P0500 [FN4A-EL].)
P0505 | IAC system problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0506 | IAC system RPM lower than expected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0507 | IAC system RPM higher than expected | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0511 | IAC circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0550 | PSP switch circuit problem | (See DTC TABLE [ZJ, Z6].)
P0602 | PCM programming error | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0610 | PCM vehicle options error | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0660 | VIS intake-air control circuit/open | (See DTC TABLE [ZJ, Z6].)
P0661 | Variable intake-air solenoid valve circuit low input | (See DTC TABLE [LF].)
P0662 | Variable intake-air solenoid valve circuit high input | (See DTC TABLE [LF].)
P0668 | PCM temperature sensor circuit low input | (See DTC TABLE [ZJ, Z6].)
P0669 | PCM temperature sensor circuit high input | (See DTC TABLE [ZJ, Z6].)
P0703 | Brake switch input circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0704 | CPP switch input circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0706 | Transaxle range (TR) switch circuit range/performance | ON | YES | 2 | CCM | X | (See DTC P0706 [FN4A-EL].)
P0707 | Transaxle range (TR) switch circuit low input | ON | YES | 1 | CCM | X | (See DTC P0707 [FN4A-EL].)
P0708 | Transaxle range (TR) switch circuit high input | ON | YES | 2 | CCM | X | (See DTC P0708 [FN4A-EL].)
P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (stuck) | ON | NO | 2 | CCM | X | (See DTC P0711 [FN4A-EL].)
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short to ground) | ON | YES | 1 | CCM | X | (See DTC P0712 [FN4A-EL].)
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | ON | YES | 1 | CCM | X | (See DTC P0713 [FN4A-EL].)
P0715 | Input/turbine speed sensor circuit malfunction | ON | YES | 1 | CCM | X | (See DTC P0715 [FN4A-EL].)
P0731 | Gear 1 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0731 [FN4A-EL].)
P0732 | Gear 2 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0732 [FN4A-EL].)
P0733 | Gear 3 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0733 [FN4A-EL].)
P0734 | Gear 4 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0734 [FN4A-EL].)
P0741 | Torque converter clutch (TCC) (stuck off) | OFF | YES | 1 | CCM | X | (See DTC P0741 [FN4A-EL].)
P0742 | Torque converter clutch (TCC) (stuck on) | OFF | YES | 1 | CCM | X | (See DTC P0742 [FN4A-EL].)
P0745 | Pressure control solenoid malfunction | OFF | YES | 1 | CCM | X | (See DTC P0745 [FN4A-EL].)
P0751 | Shift solenoid A stuck off | ON | YES | 2 | CCM | X | (See DTC P0751 [FN4A-EL].)
P0752 | Shift solenoid A stuck on | ON | YES | 2 | CCM | X | (See DTC P0752 [FN4A-EL].)
P0753 | Shift solenoid A malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0753 [FN4A-EL].)
P0756 | Shift solenoid B stuck off | ON | YES | 2 | CCM | X | (See DTC P0756 [FN4A-EL].)
P0757 | Shift solenoid B stuck on | ON | YES | 2 | CCM | X | (See DTC P0757 [FN4A-EL].)
P0758 | Shift solenoid B malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0758 [FN4A-EL].)
P0761 | Shift solenoid C stuck off | ON | YES | 2 | CCM | X | (See DTC P0761 [FN4A-EL].)
P0762 | Shift solenoid C stuck on | ON | YES | 2 | CCM | X | (See DTC P0762 [FN4A-EL].)
P0763 | Shift solenoid C malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0763 [FN4A-EL].)
P0766 | Shift solenoid D stuck off | ON | YES | 2 | CCM | X | (See DTC P0766 [FN4A-EL].)
P0767 | Shift solenoid D stuck on | ON | YES | 2 | CCM | X | (See DTC P0767 [FN4A-EL].)
P0768 | Shift solenoid D malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0768 [FN4A-EL].)
P0771 | Shift solenoid E stuck off | ON | YES | 2 | CCM | X | (See DTC P0771 [FN4A-EL].)
P0772 | Shift solenoid E stuck on | ON | YES | 2 | CCM | X | (See DTC P0772 [FN4A-EL].)
P0773 | Shift solenoid E malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0773 [FN4A-EL].)
P0850 | Neutral switch input circuit problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P0894 | Forward clutch torque transmission | OFF | Yes | 1 | CCM | X | (See DTC P0894 [FN4A-EL].)
P1260 | Immobilizer system problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2006 | Variable tumble control stuck close | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2008 | Variable tumble control circuit/open | (See DTC TABLE [ZJ, Z6].)
P2088 | Variable valve timing control circuit low | (See DTC TABLE [ZJ, Z6].)
P2089 | Variable valve timing control circuit high | (See DTC TABLE [ZJ, Z6].)
P2096 | Target A/F feedback system too lean | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2097 | Target A/F feedback system too rich | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2177 | System too lean off idle | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2178 | System too rich off idle | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2187 | System too lean at idle | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2188 | System too rich at idle | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2195 | Front HO2S signal stuck lean | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2196 | Front HO2S signal stuck rich | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2228 | BARO sensor circuit low input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2229 | BARO sensor circuit high input | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2502 | Charging system voltage problem | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2503 | Charging system voltage low | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2504 | Charging system voltage high | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
P2507 | PCM power input signal low | (See DTC TABLE [ZJ, Z6].) (See DTC TABLE [LF].)
U0073 | Control module communication bus off | (See MULTIPLEX COMMUNICATION SYSTEM.)
U0121 | Lost communication with anti-lock brake system (ABS) control module | (See MULTIPLEX COMMUNICATION SYSTEM.)
U0155 | Lost communication with instrument panel cluster (IPS) control module | (See MULTIPLEX COMMUNICATION SYSTEM.)

  * :
LF