DTC TABLE [PJB]

#
DTC TABLE [PJB]

B3E090201072W02

DTC table

DTC No. | Description | Detection condition | Page
--- | --- | --- | ---
B1002 | Auto leveling function failure | Open circuit or short to power supply in wiring harness between PJB and auto leveling control control module | (See DTC B1002.)
B1014 | Rain sensor error | Rain sensor internal malfunction | (See DTC B1014.)
B1311 | Unlock switch circuit open | Open circuit in wiring harness between PJB and driver-side door lock-link switch (unlock signal) | (See DTC B1311.)
B1317 | Battery voltage high | Input voltage from the battery is excessively high | (See DTC B1317.)
B1318 | Battery voltage low | Input voltage from the battery is excessively low | (See DTC B1318.)
B1320 | Door ajar LF circuit open | Open circuit in wiring harness between PJB and front door latch switch (driver-side) | (See DTC B1320.)
B1328 | Door ajar RF circuit open | Open circuit in wiring harness between PJB and front door latch switch (passenger-side) | (See DTC B1328.)
B1336 | Door ajar RR circuit open | Open circuit in wiring harness between PJB and rear door latch switch (RH) | (See DTC B1336.)
B1342 | ECU is faulted | PJB microcomputer malfunction | (See DTC B1342.)
B1345 | Heated backlite input circuit short to ground | Short to GND in wiring harness between PJB and climate control unit (rear window defroster switch) | (See DTC B1345.)
B1350 | Heated backlite relay short to ground | Short to GND or power supply in wiring harness between PJB and rear window defroster relay | (See DTC B1350.)
B1447 | Wiper park sense circuit open | Open circuit in wiring harness between PJB and windshield wiper motor (autostop switch) | (See DTC B1447.)
B1472 | Headlight on status switch input circuit short to ground | Short to GND in wiring harness between PJB and light switch (low beam) | (See DTC B1472.)
B1502 | Light turn signal left circuit short to ground | Short to GND in wiring harness between PJB and turn lights | (See DTC B1502.)
B1506 | Light turn signal right circuit short to ground | Short to GND in wiring harness between PJB and turn switch | (See DTC B1506.)
B1520 | Bonnet latch switch circuit open | Open circuit in wiring harness between PJB and bonnet latch switch | (See DTC B1520.)
B1547 | Power window-suspend control output circuit failure | Open circuit or short to power supply or GND in wiring harness between PJB and power window main switch | (See DTC B1547.)
B1554 | Decklid release circuit short to ground | Short to GND in wiring harness between PJB and trunk lid key cylinder push switch | (See DTC B1554.)
B1570 | Headlight high beam status input circuit short to battery | Short to power supply in wiring harness between PJB and light switch (high beam) | (See DTC B1570.)
B1572 | Door ajar LR circuit open | Open circuit in wiring harness between PJB and rear door latch switch (LH) | (See DTC B1572.)
B1607 | Key illumination circuit short to battery | Short to power supply in wiring harness between PJB and key illumination | (See DTC B1607.)
B1614 | Rear wiper interval switch input circuit short to ground | Short to GND in wiring harness between PJB and rear wiper and washer switch (INT) | (See DTC B1614.)
B1696 | Auto light switch input circuit short to ground | Short to GND in wiring harness between PJB and light switch (AUTO) | (See DTC B1696.)
B1798 | Position lights switch (TNS) input circuit short to ground | Short to GND in wiring harness between PJB and light switch (TNS) | (See DTC B1798.)
B1812 | Backup light switch input circuit short to battery | Short to power supply in wiring harness between PJB and back-up light switch | (See DTC B1812.)
B1873 | Turn signal/hazard power feed circuit short to ground | Short to GND in wiring harness between PJB and hazard warning switch | (See DTC B1873.)
B2060 | Heated backlite indicator circuit failure | Short to power supply in wiring harness between PJB and climate control unit (rear window defroster indicator) | (See DTC B2060.)
B2095 | Reset switch circuit failure | Short to GND in wiring harness between PJB and driver-side door key cylinder switch (unlock) | (See DTC B2095.)
B2096 | Set switch circuit failure | Short to GND in wiring harness between PJB and driver-side door key cylinder switch (lock) | (See DTC B2096.)
B2114 | Front washer switch input circuit short to battery | Short to power supply in wiring harness between PJB and windshield wiper and washer switch (front washer) | (See DTC B2114.)
B2175 | A/C request signal circuit short to ground | Short to GND in wiring harness between PJB and climate control unit (A/C ON request) | (See DTC B2175.)
B2177 | Intruder sensor circuit failure | Intruder sensor malfunction or circuit malfunction | (See DTC B2177.)
B2180 | Front wiper switch (slow) circuit short to ground | Short to GND in wiring harness between PJB and windshield wiper and washer switch (low) | (See DTC B2180.)
B2181 | Front wiper switch (fast) circuit short to ground | Short to GND in wiring harness between PJB and windshield wiper and washer switch (high) | (See DTC B2181.)
B2212 | Panel light control circuit failure | Input voltage from the panel light control switch is excessively low or high | (See DTC B2212.)
B2254 | Front fog light switch failure | Short to GND in wiring harness between PJB and fog light switch | (See DTC B2254.)
B2258 | Headlight washer relay circuit short to battery | Open circuit or short to power supply or GND in wiring harness between PJB and headlight cleaner relay | (See DTC B2258.)
B2259 | Front wiper variable intermittent switch circuit failure | Input voltage from the windshield wiper and washer switch (INT volume or sensitivity adjustment volume) is excessively low or high | (See DTC B2259.)
B2259 | Intermittent wiper circuit short to ground | Short to GND in wiring harness between PJB and windshield wiper and washer switch (INT) | (See DTC B2259.)
B2259 | Trunk lid lock/unlock switch circuit failure | Short to GND in wiring harness between PJB and trunk lid key cylinder switch | (See DTC B2259.)
B2264 | Rear fog light switch short to ground | Short to GND in wiring harness between PJB and rear fog light switch | (See DTC B2264.)
B2477 | Module configuration failure | PJB data configuration error | (See DTC B2477.)
B2479 | Park brake switch circuit open | Open circuit in wiring harness between PJB and parking brake switch | (See DTC B2479.)
B2555 | Dome light output circuit short to battery | Short to power supply in wiring harness between PJB and interior lights | (See DTC B2555.)
B2574 | Driver door lock switch short to ground | Short to GND in wiring harness between PJB and driver-side door lock-link switch | (See DTC B2574.)
B2665 | Battery back sounder circuit failure | Short to power in wiring harness between PJB and theft-deterrent siren | (See DTC B2665.)
B2694 | Intrusion power output failure | Short to power supply or GND in wiring harness between PJB and intruder sensor | (See DTC B2694.)
B2721 | Liftgate/decklid ajar output short to ground | Short to GND in wiring harness between PJB and trunk lid latch switch/liftgate latch switch | (See DTC B2721.)
B2840 | Ambient air thermistor circuit failure | Open circuit or short to power supply or GND in wiring harness between PJB and ambient temperature sensor | (See DTC B2840.)
B2897 | Auto light relay circuit failure | Short to power supply in PJB internal circuit between microcomputer and headlight LO relay | (See DTC B2897.)
B2898 | Right turn signal indicator output failure | • Open circuit or short to power supply or GND in wiring harness between PJB and turn light • Turn light bulb malfunction | (See DTC B2898.)
B2899 | Left turn signal indicator output failure | • Open circuit or short to power supply or GND in wiring harness between PJB and turn light • Turn light bulb malfunction | (See DTC B2899.)
B2966 | Front washer switch stuck | Windshield washer switch stuck ON position | (See DTC B2966.)
B2968 | Battery back sounder circuit short to ground | Short to GND in wiring harness between PJB and theft-deterrent siren | (See DTC B2968.)
B2973 | Running light relay circuit failure | Short to power supply or GND in PJB internal circuit between microcomputer and running light relay | (See DTC B2973.)
C1189 | Brake fluid level sensor input circuit open | Open circuit in wiring harness between PJB and brake fluid level sensor | (See DTC C1189.)
P0071 | Ambient air temperature sensor range/performance | Input voltage from the ambient temperature sensor is excessively low or high | (See DTC P0071.)
U2030 | Rain sensor communication fault | Communication error to rain sensor | (See DTC U2030.)