REAR BELTLINE MOLDING REMOVAL/INSTALLATION

#
REAR BELTLINE MOLDING REMOVAL/INSTALLATION

B3E091650641W02

1. Remove the sail garnish. (See SAIL GARNISH REMOVAL/INSTALLATION.)

2. Remove the rear door garnish. (See REAR DOOR GARNISH REMOVAL/INSTALLATION.)

3. Raise the center of the rear beltline molding and detach tabs A.

4. Using a small flathead screwdriver, detach clip B and remove the rear beltline molding.

5. Install in the reverse order of removal.