REAR WASHER HOSE REMOVAL/INSTALLATION

#
REAR WASHER HOSE REMOVAL/INSTALLATION

B3E091967470W01

1. Disconnect the negative battery cable.

2. Slightly bend back the mudguard (RH).

3. Disconnect the rear washer hose A from the washer tank.

4. Remove rear washer hose A from clips A.

5. Remove A-pillar trim (RH). (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

6. Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION)

7. Remove the dashboard garnish. (See DASHBOARD GARNISH REMOVAL/INSTALLATION)

8. Disconnect joint pipe, then remove the rear washer hose A.

9. Remove rear washer hose B from the clips B.

10. Remove the following parts:

  (1) Upper anchor of the front seat belt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)
  (2) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (4) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)
  (5) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)
  (6) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (7) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (8) Trunk side upper trim (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION.)
  (9) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)
  (10) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (11) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (12) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (13) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

11. Disconnect the joint pipe B.

12. Remove the headliner. (See HEADLINER REMOVAL/INSTALLATION)

13. Remove rear washer hose B and the tapes.

14. Remove clips C from the body.

15. Disconnect the joint pipe C, then remove rear washer hose C.

16. Remove rear washer hose D from the rear washer nozzle.

17. Install in the reverse order of removal.