DTC TABLE [ZJ, Z6]

#
DTC TABLE [ZJ, Z6]

B3E010200102W22
×: Applicable
-: Not applicable

DTC No. | Condition | MIL | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | ---
P0011 | CMP-timing over-advanced | ON | 1 | CCM | × | (See DTC P0011 [ZJ, Z6].)
P0012 | CMP-timing over-retarded | ON | 2 | CCM | × | (See DTC P0012 [ZJ, Z6].)
P0031 | Front HO2S heater control circuit low | ON | 2 | HO2S heater | × | (See DTC P0031 [ZJ, Z6].)
P0032 | Front HO2S heater control circuit high | ON | 2 | HO2S heater | × | (See DTC P0032 [ZJ, Z6].)
P0037 | Rear HO2S heater control circuit low | ON | 2 | HO2S heater | × | (See DTC P0037 [ZJ, Z6].)
P0038 | Rear HO2S heater control circuit high | ON | 2 | HO2S heater | × | (See DTC P0038 [ZJ, Z6].)
P0102 | MAF sensor circuit low input | ON | 1 | CCM | × | (See DTC P0102 [ZJ, Z6].)
P0103 | MAF sensor circuit high input | ON | 1 | CCM | × | (See DTC P0103 [ZJ, Z6].)
P0111 | IAT sensor circuit range/performance problem | ON | 2 | CCM | × | (See DTC P0111 [ZJ, Z6].)
P0112 | IAT sensor circuit low input | ON | 1 | CCM | × | (See DTC P0112 [ZJ, Z6].)
P0113 | IAT sensor circuit high input | ON | 1 | CCM | × | (See DTC P0113 [ZJ, Z6].)
P0117 | ECT sensor circuit low input | ON | 1 | CCM | × | (See DTC P0117 [ZJ, Z6].)
P0118 | ECT sensor circuit high input | ON | 1 | CCM | × | (See DTC P0118 [ZJ, Z6].)
P0121 | TP sensor circuit range/performance problem | ON | 2 | CCM | × | (See DTC P0121 [ZJ, Z6].)
P0122 | TP sensor circuit low input | ON | 1 | CCM | × | (See DTC P0122 [ZJ, Z6].)
P0123 | TP sensor circuit high input | ON | 1 | CCM | × | (See DTC P0123 [ZJ, Z6].)
P0125 | Insufficient coolant temperature for closed loop fuel control | ON | 2 | CCM | × | (See DTC P0125 [ZJ, Z6].)
P0132 | Front HO2S circuit high voltage | ON | 2 | HO2S | × | (See DTC P0132 [ZJ, Z6].)
P0133 | Front HO2S circuit slow response | ON | 2 | HO2S | × | (See DTC P0133 [ZJ, Z6].)
P0134 | Front HO2S circuit no activity detected | ON | 2 | HO2S | × | (See DTC P0134 [ZJ, Z6].)
P0138 | Rear HO2S circuit high voltage | ON | 2 | HO2S | × | (See DTC P0138 [ZJ, Z6].)
P0140 | Rear HO2S circuit no activity detected | ON | 2 | HO2S | × | (See DTC P0140 [ZJ, Z6].)
P0300 | Random misfire detected | Flash/ON | 2 | Misfire | × | (See DTC P0300 [ZJ, Z6].)
P0301 | Cylinder No.1 misfire detected | Flash/ON | 2 | Misfire | × | (See DTC P0301, P0302, P0303, P0304 [ZJ, Z6].)
P0302 | Cylinder No.2 misfire detected | Flash/ON | 2 | Misfire | × | (See DTC P0301, P0302, P0303, P0304 [ZJ, Z6].)
P0303 | Cylinder No.3 misfire detected | Flash/ON | 2 | Misfire | × | (See DTC P0301, P0302, P0303, P0304 [ZJ, Z6].)
P0304 | Cylinder No.4 misfire detected | Flash/ON | 2 | Misfire | × | (See DTC P0301, P0302, P0303, P0304 [ZJ, Z6].)
P0327 | KS circuit low input | ON | 1 | CCM | × | (See DTC P0327 [ZJ, Z6].)
P0328 | KS circuit high input | ON | 1 | CCM | × | (See DTC P0328 [ZJ, Z6].)
P0335 | CKP sensor circuit problem | ON | 1 | CCM | × | (See DTC P0335 [ZJ, Z6].)
P0340 | CMP sensor circuit problem | ON | 1 | CCM | × | (See DTC P0340 [ZJ, Z6].)
P0403 | EGR control circuit problem | ON | 2 | CCM | × | (See DTC P0403 [ZJ, Z6].)
P0420 | Catalyst system efficiency below threshold | ON | 2 | Catalyst | × | (See DTC P0420 [ZJ, Z6].)
P0443 | Purge solenoid valve circuit problem | ON | 2 | CCM | × | (See DTC P0443 [ZJ, Z6].)
P0480 | Cooling fan control circuit problem | OFF | 1 | Other | × | (See DTC P0480 [ZJ, Z6].)
P0500 | VSS circuit problem | ON | 2 | CCM | × | (See DTC P0500 [ZJ, Z6].)
P0505 | IAC system problem | OFF | - | - | - | (See DTC P0505 [ZJ, Z6].)
P0506 | IAC system RPM lower than expected | ON | 2 | CCM | × | (See DTC P0506 [ZJ, Z6].)
P0507 | IAC system RPM higher than expected | ON | 2 | CCM | × | (See DTC P0507 [ZJ, Z6].)
P0511 | IAC circuit problem | ON | 1 | CCM | × | (See DTC P0511 [ZJ, Z6].)
P0550 | PSP switch circuit problem | ON | 2 | CCM | × | (See DTC P0550 [ZJ, Z6].)
P0602 | PCM programming error | ON | 1 | CCM | × | (See DTC P0602 [ZJ, Z6].)
P0610 | PCM vehicle options error | ON | 1 | CCM | × | (See DTC P0610 [ZJ, Z6].)
P0660*1 | Variable intake-air control circuit/open | OFF | 1 | Other | × | (See DTC P0660 [Z6].)
P0668 | PCM temperature sensor circuit low input | OFF | 1 | Other | × | (See DTC P0668 [ZJ, Z6].)
P0669 | PCM temperature sensor circuit high input | OFF | 1 | Other | × | (See DTC P0669 [ZJ, Z6].)
P0703 | Brake switch input circuit problem | ON | 2 | CCM | × | (See DTC P0703 [ZJ, Z6].)
P0704 | CPP switch input circuit problem | ON | 2 | CCM | × | (See DTC P0704 [ZJ, Z6].)
P0706 | Transaxle range (TR) switch circuit range/performance | (See DTC TABLE [FN4A-EL].)
P0707 | Transaxle range (TR) switch circuit low input | (See DTC TABLE [FN4A-EL].)
P0708 | Transaxle range (TR) switch circuit high input | (See DTC TABLE [FN4A-EL].)
P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (stuck) | (See DTC TABLE [FN4A-EL].)
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short to ground) | (See DTC TABLE [FN4A-EL].)
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | (See DTC TABLE [FN4A-EL].)
P0715 | Input/turbine speed sensor circuit malfunction | (See DTC TABLE [FN4A-EL].)
P0731 | Gear 1 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0732 | Gear 2 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0733 | Gear 3 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0734 | Gear 4 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0741 | Torque converter clutch (TCC) (stuck off) | (See DTC TABLE [FN4A-EL].)
P0742 | Torque converter clutch (TCC) (stuck on) | (See DTC TABLE [FN4A-EL].)
P0745 | Pressure control solenoid malfunction | (See DTC TABLE [FN4A-EL].)
P0751 | Shift solenoid A stuck off | (See DTC TABLE [FN4A-EL].)
P0752 | Shift solenoid A stuck on | (See DTC TABLE [FN4A-EL].)
P0753 | Shift solenoid A malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0756 | Shift solenoid B stuck off | (See DTC TABLE [FN4A-EL].)
P0757 | Shift solenoid B stuck on | (See DTC TABLE [FN4A-EL].)
P0758 | Shift solenoid B malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0761 | Shift solenoid C stuck off | (See DTC TABLE [FN4A-EL].)
P0762 | Shift solenoid C stuck on | (See DTC TABLE [FN4A-EL].)
P0763 | Shift solenoid C malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0766 | Shift solenoid D stuck off | (See DTC TABLE [FN4A-EL].)
P0767 | Shift solenoid D stuck on | (See DTC TABLE [FN4A-EL].)
P0768 | Shift solenoid D malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0771 | Shift solenoid E stuck off | (See DTC TABLE [FN4A-EL].)
P0772 | Shift solenoid E stuck on | (See DTC TABLE [FN4A-EL].)
P0773 | Shift solenoid E malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0850 | Neutral switch input circuit problem | ON | 2 | CCM | × | (See DTC P0850 [ZJ, Z6].)
P0894 | Forward clutch torque transmission | (See DTC TABLE [FN4A-EL].)
P1260 | Immobilizer system problem | OFF | - | Other | - | (See DTC P1260 [ZJ, Z6].)
P2006 | Variable tumble control stuck close | ON | 2 | CCM | × | (See DTC P2006 [ZJ, Z6].)
P2008 | Variable tumble control circuit/open | ON | 2 | CCM | × | (See DTC P2008 [ZJ, Z6].)
P2088 | Variable valve timing control circuit low | ON | 1 | CCM | × | (See DTC P2088 [ZJ, Z6].)
P2089 | Variable valve timing control circuit high | ON | 1 | CCM | × | (See DTC P2089 [ZJ, Z6].)
P2096 | Target A/F feedback system too lean | ON | 2 | Fuel system | × | (See DTC P2096 [ZJ, Z6].)
P2097 | Target A/F feedback system too rich | ON | 2 | Fuel system | × | (See DTC P2097 [ZJ, Z6].)
P2177 | System too lean off idle | ON | 2 | Fuel system | × | (See DTC P2177 [ZJ, Z6].)
P2178 | System too rich off idle | ON | 2 | Fuel system | × | (See DTC P2178 [ZJ, Z6].)
P2187 | System too lean at idle | ON | 2 | Fuel system | × | (See DTC P2187 [ZJ, Z6].)
P2188 | System too rich at idle | ON | 2 | Fuel system | × | (See DTC P2188 [ZJ, Z6].)
P2195 | Front HO2S signal stuck lean | ON | 2 | HO2S | × | (See DTC P2195 [ZJ, Z6].)
P2196 | Front HO2S signal stuck rich | ON | 2 | HO2S | × | (See DTC P2196 [ZJ, Z6].)
P2228 | BARO sensor circuit low input | ON | 1 | CCM | × | (See DTC P2228 [ZJ, Z6].)
P2229 | BARO sensor circuit high input | ON | 1 | CCM | × | (See DTC P2229 [ZJ, Z6].)
P2502 | Charging system voltage problem | OFF | 1 | - | - | (See DTC P2502 [ZJ, Z6].)
P2503 | Charging system voltage low | OFF | 1 | - | - | (See DTC P2503 [ZJ, Z6].)
P2504 | Charging system voltage high | OFF | 1 | - | - | (See DTC P2504 [ZJ, Z6].)
P2507 | PCM power input signal low | ON | 1 | CCM | × | (See DTC P2507 [ZJ, Z6].)
U0073 | Control module communication bus off | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)
U0121 | Lost communication with anti-lock brake system (ABS) control module | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)
U0155 | Lost communication with instrument panel cluster (IPC) control module | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)

  *1 :
Z6