DTC P0117 [LF]

#
DTC P0117 [LF]

B3E010201084W13

DTC P0117 | ECT sensor circuit low input
--- | ---

DETECTION CONDITION

• The PCM monitors the ECT sensor signal at PCM terminal 2AK. If the PCM detects the ECT sensor voltage below 0.2 V, the PCM determines that the ECT sensor circuit has malfunction.
Diagnostic support note
• This is a continuous monitor (CCM).
• The MIL illuminates if the PCM detects the above malfunction condition during first drive cycle.
• PENDING CODE is available if the PCM detects the above malfunction condition.
• FREEZE FRAME DATA is available.
• The DTC is stored in the PCM memory.

POSSIBLE CAUSE | • ECT sensor malfunction • Connect or terminal malfunction • Short to ground in wiring harness between ECT sensor terminal A and PCM connector terminal 2AK • Short each wiring harness ECT signal circuit and ECT ground circuit • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT TERMINAL BENT • Turn the ignition switch off. • Disconnect the ECT sensor connector. • Inspect for bent of ECT sensor terminals A and B (part-side). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 7.
No | Go to the next step.
4 | CLASSIFY ECT SENSOR MALFUNCTION OR WIRING HARNESS MALFUNCTION • Connect the WDS or equivalent to DLC-2. • Access ECT PID. • Verify ECT value when disconnecting ECT sensor connector. • Does the ECT value change? | Yes | Replace the ECT sensor, then go to Step 7.
No | Go to the next step.
5 | INSPECT ECT SIGNAL CIRCUIT FOR SHORT TO GROUND • Turn the ignition switch off. • Inspect continuity between ECT sensor terminal A (wiring harness-side) and body ground. • Is there continuity? | Yes | Repair or replace the wiring harness for short to ground, then go to Step 7.
No | Go to the next step.
6 | INSPECT IAT CIRCUIT FOR SHORT WIRING HARNESSES • Inspect for continuity between ECT sensor terminal A and B (wiring harness-side). • Is there continuity? | Yes | Repair or replace the wiring harness for short, then go to the next step.
No | Go to the next step.
7 | VERIFY TROUBLESHOOTING OF DTC P0117 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [LF].)
No | Go to the next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [LF].) • Are any DTC present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [LF].)
No | Troubleshooting completed.