SUNROOF UNIT REMOVAL/INSTALLATION

#
SUNROOF UNIT REMOVAL/INSTALLATION

B3E091569850W02

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Console (4SD) (See CONSOLE REMOVAL/INSTALLATION.)
  (2) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (3) Upper anchor of the front seat belt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)
  (4) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (5) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (6) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)
  (7) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)
  (8) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (9) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (10) Trunk side upper trim (5HB) (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION.)
  (11) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)
  (12) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (13) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (14) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (15) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)
  (16) Headliner (See HEADLINER REMOVAL/INSTALLATION.)
  (17) Head impact pad (See HEAD IMPACT PAD REMOVAL/INSTALLATION.)
  (18) Glass panel (See GLASS PANEL REMOVAL/INSTALLATION.)

3. Disconnect the front and rear drain hoses from the sunroof frame.

4. Remove the bolts and nuts, then remove the sunroof unit.

5. Install in the reverse order of removal.

6. Adjust the glass panel. (See GLASS PANEL ADJUSTMENT.)