COWL GRILLE REMOVAL/INSTALLATION

#
COWL GRILLE REMOVAL/INSTALLATION

B3E091650780W01

1. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Using a small flathead screwdriver, remove the caps.

3. Remove the screws.

4. Remove the weatherstrip.

5. Move the cowl grille in the direction indicated by the arrow and disengage tabs A from the windshield.

6. Remove the cowl grille.

7. Install in the reverse order of removal.