BRAKE FLUID PRESSURE SENSOR INITIALIZATION PROCEDURE

#
BRAKE FLUID PRESSURE SENSOR INITIALIZATION PROCEDURE

B3E041543771W02

  Warning

  • If the initialization procedure is not completed, the DSC will not operate properly and it might cause an unexpected accident. Therefore, after replacing or removing the DSC HU/CM, make sure to perform the initialization procedure to insure proper DSC operation.

1. Turn the ignition switch off.

2. Connect the WDS or equivalent to the DLC-2.

3. Access the active command mode, then select and perform the following commands.

  - MCYL_S_CAL (brake fluid pressure sensor)

4. Drive the vehicle.

5. After 5 min or more of driving, verify that the DSC system is normal.