REAR HEAT DUCT REMOVAL/INSTALLATION

#
REAR HEAT DUCT REMOVAL/INSTALLATION

B3E071161273W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front seat (See FRONT SEAT REMOVAL/INSTALLATION.)
  (2) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (3) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (4) Console (See CONSOLE REMOVAL/INSTALLATION.)
  (5) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (6) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (7) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)
  (8) Lower anchor of the front seat belt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)
  (9) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (10) Fuel-filler lid opener lever cover (See FUEL-FILLER LID OPENER REMOVAL/INSTALLATION [L.H.D.].) (See FUEL-FILLER LID OPENER REMOVAL/INSTALLATION [R.H.D.].)
  (11) Floor covering (See FLOOR COVERING REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Rear heat duct (1)
2 | Rear heat duct (2)
3 | Rear heat duct (3)

4. Install in the reverse order of removal.