AIRFLOW MODE MAIN LINK REMOVAL/INSTALLATION

#
AIRFLOW MODE MAIN LINK REMOVAL/INSTALLATION

B3E071161130W05

## L.H.D.

1. Disconnect the negative battery cable.

2. Detach the bonnet release lever from the lower panel. (SeeBONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [L.H.D.].)

3. Remove the front scuff plate. (SeeFRONT SCUFF PLATE REMOVAL/INSTALLATION.)

4. Remove the front side trim. (SeeFRONT SIDE TRIM REMOVAL/INSTALLATION.)

5. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

6. Remove the shower duct (LH).

7. Remove the airflow mode actuator. (full-auto air conditioner) (See AIRFLOW MODE ACTUATOR REMOVAL/INSTALLATION.)

8. Disconnect the airflow mode wire. (See CLIMATE CONTROL UNIT REMOVAL [MANUAL AIR CONDITIONER].)

9. Remove the airflow mode rod (1).

10. Remove the airflow mode main link.

11. Install in the reverse order of removal.

12. Adjust the airflow mode wire. (See CLIMATE CONTROL UNIT WIRE ADJUSTMENT.)

## R.H.D.

1. Disconnect the negative battery cable.

2. Removal the following parts.

  (1) Front door (See FRONT DOOR REMOVAL/INSTALLATION.)
  (2) Ashtray panel (See CONSOLE REMOVAL/INSTALLATION.)
  (3) Console (See CONSOLE REMOVAL/INSTALLATION.)
  (4) Shift lever component (MTX) (See SHIFT MECHANISM REMOVAL/INSTALLATION.)
  (5) Selector lever component (ATX) (See SELECTOR LEVER COMPONENT REMOVAL/INSTALLATION.)
  (6) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)
  (7) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (8) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (9) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  (10) Shower ducts (LH, RH)
  (11) PJB (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)
  (12) Car-navigation unit (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)
  (13) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)
  (14) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)
  (15) Steering shaft (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)
  (16) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (17) Center panel (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)
  (18) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)
  (19) Cowl grille (See COWL GRILLE REMOVAL/INSTALLATION.)
  (20) Cowl panel (See COWL PANEL REMOVAL/INSTALLATION.)
  (21) Windshield wiper motor (See WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION.)
  (22) IDashboard (See DASHBOARD REMOVAL/INSTALLATION.)

3. Remove the airflow mode rot (1).

4. Remove the airflow mode main rink.

5. Install in the reverse order of removal.

6. Adjust the airflow mode wire. (See CLIMATE CONTROL UNIT WIRE ADJUSTMENT.)

## Airflow Mode Main Link Installation Note

  Caution

  • Apply only the specified grease to links. Otherwise abnormal noise or improper operation may result.

1. Push and hold each airflow mode sub link in the direction of the arrow.

2. Set the airflow mode main link to the A/C unit as shown in the figure.

3. Press the airflow mode main link lightly to the A/C unit it in the direction shown by the arrow, then set the projections of each airflow mode sub link into the grooves of the airflow mode main link.

4. Rotate airflow mode main link and verify that each mode is accessed properly.