DTC TABLE [IMMOBILIZER SYSTEM]

#
DTC TABLE [IMMOBILIZER SYSTEM]

B3E090201077W03

DTC | Detection condition | Page
--- | --- | ---
Security light flashing pattern | WDS or equivalent display*
Instrument cluster | PCM
11 |  | B1681 | P1260 | No detected communication with the coil | SECURITY LIGHT 11, DTC B1681/P1260
12 |  | B2103 | P1260 | • Coil antenna malfunction • The PCM determined a malfunction in the coil antenna even though it is normal. | SECURITY LIGHT 12, DTC B2103/P1260
13 |  | B1600 | P1260 | The key ID number data cannot be read. | SECURITY LIGHT 13, DTC B1600/P1260
B2431 | P1260 | Key ID number registration error | SECURITY LIGHT 13, DTC B2431/P1260
14 |  | B1602 | P1260 | The instrument cluster cannot read key ID number data normally. | SECURITY LIGHT 14, DTC B1602/P1260
15 |  | B1601 | P1260 | The instrument cluster has detected unregistered key ID number. | SECURITY LIGHT 15, DTC B1601/P1260
16 |  | U2510 | P1260 | Communication error between the instrument cluster and the PCM (no response) | SECURITY LIGHT 16, DTC U2510/P1260, U1147/P1260
U1147 | P1260 | Communication error between the instrument cluster and the PCM (mismatched conditions)
21 |  | B1213 | P1260 | Only one key ID number is registered. | SECURITY LIGHT 21, DTC B1213/P1260
22 |  | B2141 | P1260 | Communication error between the instrument cluster and the PCM (data transfer error) | SECURITY LIGHT 22, DTC B2141/P1260
23 |  | B2139 | P1260 | ID number data in the PCM and the instrument cluster do not match. | SECURITY LIGHT 23, DTC B2139/P1260
Not illuminated | B1342 | - | Instrument cluster malfunction | DTC B1342 [IMMOBILIZER SYSTEM]

  * :
The letters at the beginning of each DTC are only displayed when using the WDS or equivalent, and refer to the following: B= Body system, P= Powertrain system, U= Network communication system.