NO.1 ALC (AUTOMATIC LEVEL CONTROL) DO NOT OPERATE. (ABS HU/CM OPERATES NORMALLY.)

#
NO.1 ALC (AUTOMATIC LEVEL CONTROL) DO NOT OPERATE. (ABS HU/CM OPERATES NORMALLY.)

B3E090366900W03

1 | ALC (automatic level control) do not operate. (ABS HU/CM operates normally.)

TROUBLESHOOTING HINTS

• Malfunction in vehicle speed signal line of audio unit.

  - Audio unit malfunction
  - ABS HU/CM malfunction
  - Malfunction in wiring harness between audio unit and ABS HU/CM

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is ALC function operating? | Yes | Go to next step.
No | Make ALC function operate, then go to Step 5.
2 | • Inspect DTC of PCM. • Is DTC P0500 (VSS circuit malfunction) displayed? | Yes | Go to applicable DTC inspection.
No | Go to next step.
3* | • Disconnect audio unit connector (24-pin) and ABS HU/CM connector (28-pin). • Is there continuity between audio unit connector (24-pin) terminal 1I and ABS HU/CM connector (28-pin) terminal 1V? | Yes | Go to next step.
No | Repair wiring harness between audio unit and ABS HU/CM, then go to Step 5.
4 | • Inspect wiring harness between audio unit connector (24-pin) terminal 1I and ABS HU/CM connector (28-pin) terminal 1V for short to ground. • Is there short to ground? | Yes | Repair wiring harness between audio unit and ABS HU/CM, then go to next step.
No | Replace base unit, then go to next step.
5 | • Does ALC operate normally? | Yes | Complete troubleshooting, then explain repairs to customer.
No | Recheck malfunction symptoms, then repeat from Step 1 if malfunction recurs.