PANEL LIGHT CONTROL SWITCH REMOVAL/INSTALLATION

#
PANEL LIGHT CONTROL SWITCH REMOVAL/INSTALLATION

B3E091866600W01

1. Disconnect the negative battery cable.

2. Detach the bonnet release lever from the lower panel. (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [L.H.D.].) (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [R.H.D.].)

3. Remove the front scuff plate. (Driver's side) (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

4. Remove the front side trim. (Driver's side) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

5. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

6. Remove the panel light control switch.

7. Disconnect the panel light control switch connector.

8. Install in the reverse order of removal.