VENTILATOR GRILLE REMOVAL/INSTALLATION

#
VENTILATOR GRILLE REMOVAL/INSTALLATION

B3E091764810W01

## Driver's Side

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (2) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (4) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)
  (5) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)
  (6) Dashboard center panel (See DASHBOARD CENTER PANEL REMOVAL/INSTALLATION.)
  (7) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)
  (8) Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)
  (9) Dashboard garnish (See DASHBOARD GARNISH REMOVAL/INSTALLATION.)

3. Pull the driver-side ventilator grille outward and remove it.

4. Remove the screw, then remove the driver-side demister grille.

5. Install in the reverse order of removal.

## Passenger's Side

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (2) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (4) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  (5) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)
  (6) Dashboard center panel (See DASHBOARD CENTER PANEL REMOVAL/INSTALLATION.)
  (7) Dashboard garnish (See DASHBOARD GARNISH REMOVAL/INSTALLATION.)

3. Pull the passenger-side ventilator grille outward and remove it.

4. Remove the screw, then remove the passenger-side demister grille.

5. Install in the reverse order of removal.

## Center

1. Remove the decoration panel. (See DECORATION PANEL REMOVAL/INSTALLATION.)

2. Remove the dashboard center panel. (See DASHBOARD CENTER PANEL REMOVAL/INSTALLATION.)

3. Remove the screws, then remove the center ventilator grilles.

4. Install in the reverse order of removal.