MAGNETIC CLUTCH DISASSEMBLY/ASSEMBLY [LF]

#
MAGNETIC CLUTCH DISASSEMBLY/ASSEMBLY [LF]

B3E074061010W02

1. Disassemble in the order indicated in the table.

1 | Bolt (See Bolt Removal/Installation Note.)
2 | Pressure plate
3 | Shim
4 | Snap ring (See Snap Ring Installation Note.)
5 | A/C compressor pulley
6 | Screw (See Screw Installation Note.)
7 | Clamp (See Clamp Installation Note.)
8 | Stator and thermal protector (See Stator and Thermal Protector Removal Note.) (See Stator and Thermal Protector Installation Note.)
9 | A/C compressor body

2. Assemble in the reverse order of disassembly.

3. Adjust the magnetic clutch clearance. (See MAGNETIC CLUTCH ADJUSTMENT.)

## Bolt Removal/Installation Note

1. When removing or installing the bolt, hold the pressure plate in place as shown in the figure.

2. When installing a new A/C compressor body, replace the recommended bolt.