POWER WINDOW SUBSWITCH REMOVAL/INSTALLATION

#
POWER WINDOW SUBSWITCH REMOVAL/INSTALLATION

B3E091266330W03

1. Disconnect the negative battery cable.

2. Remove clip B using a flathead screwdriver wrapped with protective tape.

3. Remove the switch panel from the door trim while sliding it in the direction of the arrow as shown in the figure.

4. Disconnect the power window subswitch connector.

5. Remove the screws, then remove the power window subswitch.

6. Install in the reverse order of removal.