LCD UNIT REMOVAL/INSTALLATION

#
LCD UNIT REMOVAL/INSTALLATION

B3E092066901W01

1. Disconnect the negative battery cable.

2. Remove the decoration panel. (See DECORATION PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | LCD unit (See LCD Unit Removal Note.)

4. Install in the reverse order of removal.

## LCD Unit Removal Note

1. Pull the lower LCD unit outward, detach clip A and pin B from the dashboard, and then remove the LCD unit.