POWER OUTER MIRROR INSPECTION

#
POWER OUTER MIRROR INSPECTION

B3E091269110W03

1. Apply battery positive voltage to the power outer mirror terminals and inspect the operation of the power outer mirror.

  • If not as specified, replace the power outer mirror.

Mirror operation | Terminal
--- | ---
B+ | GND
Up | B | D
Down | D | B
Left | F | D
Right | D | F

2. Inspect for continuity between the power outer mirror heater terminals.

  • If not as specified, replace the power outer mirror.