DTC B1342, C1267 [ABS]

#
DTC B1342, C1267 [ABS]

B3E040243000W04

DTC | B1342, C1267 | ABS HU/CM (internal malfunction)
DETECTION CONDITION | • The ABS HU/CM on-board diagnostic function detects control module internal malfunction.
POSSIBLE CAUSE | • ABS HU/CM internal malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY NO ABS HU/CM MALFUNCTION • Clear the DTCs from the memory. (See Clearing DTCs Procedures.) • Start the engine and drive the vehicle at 10km/h {6.2 mph} or more. • Are the same DTCs present? | Yes | Replace the ABS HU/CM, then go to the next step. (See ABS HU/CM REMOVAL/INSTALLATION.)
No | Go to the next step.
2 | VERIFY THAT NO OTHER DTCS ARE PRESENT • Are any other DTCs output? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | DTC troubleshooting completed.