OIL PUMP REMOVAL/INSTALLATION [LF]

#
OIL PUMP REMOVAL/INSTALLATION [LF]

B3E011119220W02

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.
  • A vehicle that is lifted but not securely supported on safety stands is dangerous. It can slip or fall, causing death or serious injury. Never work around or under a lifted vehicle if it is not securely supported on safety stands.
  • Continuous exposure to used engine oil has caused skin cancer in laboratory mice. Protect your skin by washing with soap and water immediately after working with engine oil.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Disconnect the negative battery cable.

3. Remove the under cover and splash shield as a single unit.

4. Remove the front tire (RH).

5. Drain the engine oil. (See ENGINE OIL REPLACEMENT [LF].)

6. Remove the plug hole plate. (See PLUG HOLE PLATE REMOVAL/INSTALLATION [LF].)

7. Remove the drive belt. (See DRIVE BELT REPLACEMENT [LF].)

8. Set the coolant reserve tank out of the way.

9. Remove the A/C compressor with the pipes still connected. (See A/C COMPRESSOR REMOVAL/INSTALLATION [LF].)

10. Remove the ignition coil. (See IGNITION COIL REMOVAL/INSTALLATION [LF].)

11. Remove the spark plug. (See SPARK PLUG REMOVAL/INSTALLATION [LF].)

12. Set the accelerator cable bracket out of the way.

13. Remove the crankshaft position (CKP) sensor. (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [LF].)

14. Remove the engine front cover. (See TIMING CHAIN REMOVAL/INSTALLATION [LF].)

15. Remove the oil pan. (See OIL PAN REMOVAL/INSTALLATION [LF].)

16. Remove in the order indicated in the table.

17. Install in the reverse order of removal.

18. Refill the engine with the specified type and amount of the engine oil. (See ENGINE OIL REPLACEMENT [LF].)

19. Start the engine and inspect for oil leakage.

  • If the oil leaks, specify the faulty part and repair or replace it.

20. Inspect the oil level. (See ENGINE OIL LEVEL INSPECTION [LF].)

21. Inspect for the ignition timing and idle speed. (See ENGINE TUNE-UP [LF].)

.

1 | Oil strainer
2 | Oil pump chain guide
3 | Oil pump chain tensioner and spring component
4 | Oil pump chain
5 | Oil pump sprocket (See Oil Pump Sprocket Removal/Installation Note.)
6 | Oil pump (See Oil Pump Installation Note.)

## Oil Pump Sprocket Removal/Installation Note

1. Install the SST to the oil pump sprocket to stop the oil pump from rotating.

## Oil Pump Installation Note

1. Tighten the oil pump bolts in two steps in the order indicated in the figure.

  Tightening torque:
  1) 8-10 N·m {82-101 kgf·cm, 71-88 in·lbf}
  2) 20-25 N·m {2.1-2.5 kgf·m, 15.2-18.4 ft·lbf}