REFRIGERANT PRESSURE SWITCH REMOVAL/INSTALLATION

#
REFRIGERANT PRESSURE SWITCH REMOVAL/INSTALLATION

B3E074061503W01

1. Disconnect the negative battery cable.

2. Discharge the refrigerant from the system. (See REFRIGERANT RECOVERY.) (See REFRIGERANT CHARGING.)

3. Loosen the refrigerant pressure switch using two spanners.

4. Remove in the order indicated in the table.

L.H.D.

R.H.D.

1 | Refrigerant pressure switch connector
2 | Refrigerant pressure switch (See Refrigerant Pressure Switch Installation Note.)

5. Install in the reverse order of removal.

## Refrigerant Pressure Switch Installation Note

1. Apply compressor oil to O-ring and connect the joint.