COIL ANTENNA REMOVAL/INSTALLATION

#
COIL ANTENNA REMOVAL/INSTALLATION

B3E091467002W01

  Note

  • Do not remove the coil antenna unless you are replacing it.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Bonnet release lever (SeeBONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [L.H.D.].) (SeeBONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [R.H.D.].)
  (2) Front scuff plate (Driver's side) (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) Front side trim (Driver's side) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (4) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)
  (5) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Disconnect the coil antenna connector.

4. Detach the steering lock tabs from the holes on the coil antenna.

5. Install in the reverse order of removal.