INPUT/TURBINE SPEED SENSOR INSPECTION

#
INPUT/TURBINE SPEED SENSOR INSPECTION

B3E051719010W03

  Caution

  • Water or foreign material entering the connector can cause a poor connection or corrosion. Be sure not to drop water or foreign material on the connector when disconnecting it.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Disconnect the negative battery cable.

3. Remove the battery, battery box and battery tray. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

4. Disconnect the input/turbine speed sensor connector.

5. Measure the resistance between the input/turbine speed sensor terminals.

  • If there is any malfunction, replace the input/turbine speed sensor.

  Resistance
  250-600 ohms (ATF temperature:
  -40-160 °C {-40-320 °F})

6. Connect the input/turbine speed sensor connector.

7. Install the battery, battery box and battery tray. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

8. Connect the negative battery cable.

9. Install the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)