DTC P0711 [FN4A-EL]

#
DTC P0711 [FN4A-EL]

B3E050219090W10

DTC P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (stuck)
--- | ---

DETECTION CONDITION

• When all conditions below are satisfied.

  - When 180 s have passed after the engine is started, vehicle is driven for 150 s or more at vehicle speed between 25-59 km/h {15-36 mph}, then 60 km/h {37 mph} or more for 100 s or more.
  - P0712, P0713 not output
  - Variation in ATF voltage below 0.06 V

Diagnostic support note:
• This is a continuous monitor (CCM).
• The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• The PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle.
• FREEZE FRAME DATA is available.
• AT warning light does not illuminates.
• The DTC is stored in the PCM memory.

POSSIBLE CAUSE | • TFT sensor malfunction • Connector corrosion • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has the FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Bulletins and/or on-line repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.

3

INSPECT TFT SENSOR VOLTAGE
• Turn the ignition switch to the ON position (engine off).
• Measure the voltage at PCM terminal 1AU (Z6)/1U (LF).
• Record terminal 1AU (Z6)/1U (LF) voltage.
• Start the engine.
• Drive the vehicle at 60 km/h {37 mph} or more for 430 s or more.
• Record terminal 1AU (Z6)/1U (LF) voltage again.
• Is the variation in voltage 0.06 V or more?

Yes

Go to Step 5.

No | Go to the next step.
4 | INSPECT TERMINAL CONDITION • Turn the ignition switch to the LOCK position. • Disconnect the ATX connector. • Inspect terminals for corrosion. • Are terminals normal? | Yes | Go to the next step.
No | Repair or replace the terminals, then go to the next step.

5

VERIFY TROUBLESHOOTING OF DTC P0711 COMPLETED
• Make sure to reconnect all the disconnected connectors.
• Clear the DTC from the memory using the WDS or equivalent.
• Decrease ATF temperature to 20 °C {68 °F} or less.
• Start the engine and wait for 180 s or more.
• Drive the vehicle at a vehicle speed between 25-59 km/h {15-36 mph} for 150 s or more.
• Drive the vehicle at a vehicle speed 60 km/h {37 mph} or more for 100 s or more.
• Is the PENDING CODE present?

Yes

Replace the PCM, then go to the next step.
(See PCM REMOVAL/INSTALLATION [ZJ, Z6].)
(See PCM REMOVAL/INSTALLATION [LF].)

No | Go to the next step.
6 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [FN4A-EL].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection.
No | DTC troubleshooting completed.