HIGH-MOUNT BRAKE LIGHT REMOVAL/INSTALLATION

#
HIGH-MOUNT BRAKE LIGHT REMOVAL/INSTALLATION

B3E091851580W01

## 4SD

1. Disconnect the negative battery cable.

2. Remove the trunk lid trim. (See TRUNK LID TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Connector
2 | Socket
3 | High-mount brake light bulb
4 | Nut
5 | High-mount brake light

4. Install in the reverse order of removal.

## 5HB

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Connector
2 | Socket
3 | High-mount brake light bulb
4 | High-mount brake light

4. Install in the reverse order of removal.