DRIVE BELT AUTO TENSIONER INSPECTION [ZJ, Z6]

#
DRIVE BELT AUTO TENSIONER INSPECTION [ZJ, Z6]

B3E011015800W04

1. Remove the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, Z6].)

2. Verify that the drive belt auto tensioner moves smoothly in the operational direction.

  • If it does not move smoothly, replace the drive belt auto tensioner.

3. Rotate the drive belt auto tensioner pulley by hand and verify that it rotates smoothly.

  • If it does not move smoothly, replace the drive belt auto tensioner.

4. Install the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, Z6].)