FRONT LOWER ARM INSPECTION

#
FRONT LOWER ARM INSPECTION

B3E021334300W02

1. Remove the lower arm from the vehicle.

2. Inspect the arm for bending or damage, and the ball joint for excessive looseness.

  • If there is any malfunction, replace the lower arm.

3. Rotate the ball joint stud 5 times. Install the SST to the ball joint stud, measure the rotational torque using a pull scale.

  • If not within the specification, replace the lower arm.

  Rotational torque
  1.0-4.9 N·m {11-49 kgf·cm, 9-43 in·lbf}
  Pull scale reading [10-49 N {1.1-4.9 kgf, 3-10 lbf}]