CLOCK SPRING INSPECTION

#
CLOCK SPRING INSPECTION

B3E081066123W03

1. Remove the clock spring. (See CLOCK SPRING REMOVAL/INSTALLATION.)

2. Verify that the continuity is as indicated in the table.

  • If not as indicated in the table, replace the clock spring.

  Note

  • When the vehicle-side connector for the clock spring is disconnected, terminals 1F, 1H, 1J and 1L are shorted to prevent unexpected operation (deployment) of the air bag module.