DTC TABLE

#
DTC TABLE

B3E080201046W05

DTC | System malfunction location | Page
--- | --- | ---
WDS display
B1046 | Driver-side curtain air bag module and other air bag module circuits short | (See DTC B1046, B2773, B2774, B2775, B2776.)
B1047 | Driver-side side air bag module and other air bag module circuits short | (See DTC B1047, B1992, B1993, B1994, B1995.)
B1048 | Passenger-side air bag module (inflator No.1) and other air bag module circuits short | (See DTC B1048, B1925, B1933, B1935, B1938.)
B1049 | Passenger-side pre-tensioner front buckle and other air bag module circuits short | (See DTC B1049, B1881, B1882, B1883, B1886.)
B104B | Driver-side side air bag sensor and other sensor circuits short to power supply | (See DTC B104B, B104E, B1051, U2017.)
B104C | Passenger-side side air bag sensor and other sensor circuits short to power supply | (See DTC B104C, B104F, B1050, U2018.)
B104D | Crash zone sensor and other sensor circuits short to power supply | (See DTC B104D, B2226, B2227, B2855.)
B104E | Driver-side side air bag sensor circuit open or short | (See DTC B104B, B104E, B1051, U2017.)
B104F | Passenger-side side air bag sensor (internal circuit abnormal) | (See DTC B104C, B104F, B1050, U2018.)
B1050 | Passenger-side side air bag sensor circuit open or short
B1051 | Driver-side side air bag sensor (internal circuit abnormal) | (See DTC B104B, B104E, B1051, U2017.)
B1053 | Driver-side front buckle switch and other sensor circuits short to power supply | (See DTC B1053, B2432, B2433, B2434, B2435.)
B1054 | Driver-side pre-tensioner front buckle and other air bag module circuits short | (See DTC B1054, B1877, B1878, B1879, B1885.)
B1055 | Passenger-side side air bag module and other air bag module circuits short | (See DTC B1055, B1996, B1997, B1998, B1999.)
B1056 | Passenger-side curtain air bag module and other air bag module circuits short | (See DTC B1056, B2777, B2778, B2779, B2780.)
B1057 | Driver-side air bag module (inflator No.1) and other air bag module circuits short | (See DTC B1057, B1916, B1932, B1934, B1936.)
B1058 | Driver-side air bag module (inflator No.2) and other air bag module circuits short | (See DTC B1058, B2228, B2230, B2232, B2234.)
B1059 | Passenger-side air bag module (inflator No.2) and other air bag module circuits short | (See DTC B1059, B2229, B2231, B2233, B2235.)
B105A | SAS control module activation (deployment) control frequency error | (See DTC B105A.)
B1231 | SAS control module activation (deployment) control freeze | (See DTC B1231.)
B1317 | SAS control module power supply voltage increases (16.1 V or more) | (See DTC B1317, B1318.)
B1318 | SAS control module power supply voltage decreases (less than 9 V)
B1342 | SAS control module | (See DTC B1342.)
B1877 | Driver-side pre-tensioner front buckle circuit resistance high | (See DTC B1054, B1877, B1878, B1879, B1885.)
B1878 | Driver-side pre-tensioner front buckle circuit short to power supply
B1879 | Driver-side pre-tensioner front buckle circuit short to body ground
B1881 | Passenger-side pre-tensioner front buckle circuit resistance high | (See DTC B1049, B1881, B1882, B1883, B1886.)
B1882 | Passenger-side pre-tensioner front buckle circuit short to power supply
B1883 | Passenger-side pre-tensioner front buckle circuit short to body ground
B1884 | Passenger air bag deactivation (PAD) indicator circuit open or short to body ground | (See DTC B1884, B1890.)
B1885 | Driver-side pre-tensioner front buckle circuit resistance low | (See DTC B1054, B1877, B1878, B1879, B1885.)
B1886 | Passenger-side pre-tensioner front buckle circuit resistance low | (See DTC B1049, B1881, B1882, B1883, B1886.)
B1890 | Passenger air bag deactivation (PAD) indicator circuit short to power supply | (See DTC B1884, B1890.)
B1916 | Driver-side air bag module (inflator No.1) circuit short to power supply | (See DTC B1057, B1916, B1932, B1934, B1936.)
B1925 | Passenger-side air bag module (inflator No.1) circuit short to power supply | (See DTC B1048, B1925, B1933, B1935, B1938.)
B1932 | Driver-side air bag module (inflator No.1) circuit resistance high | (See DTC B1057, B1916, B1932, B1934, B1936.)
B1933 | Passenger-side air bag module (inflator No.1) circuit resistance high | (See DTC B1048, B1925, B1933, B1935, B1938.)
B1934 | Driver-side air bag module (inflator No.1) circuit resistance low | (See DTC B1057, B1916, B1932, B1934, B1936.)
B1935 | Passenger-side air bag module (inflator No.1) circuit resistance low | (See DTC B1048, B1925, B1933, B1935, B1938.)
B1936 | Driver-side air bag module (inflator No.1) circuit short to body ground | (See DTC B1057, B1916, B1932, B1934, B1936.)
B1938 | Passenger-side air bag module (inflator No.1) circuit short to body ground | (See DTC B1048, B1925, B1933, B1935, B1938.)
B1992 | Driver-side side air bag module circuit short to power supply | (See DTC B1047, B1992, B1993, B1994, B1995.)
B1993 | Driver-side side air bag module circuit short to body ground
B1994 | Driver-side side air bag module circuit resistance high
B1995 | Driver-side side air bag module circuit resistance low
B1996 | Passenger-side side air bag module circuit short to power supply | (See DTC B1055, B1996, B1997, B1998, B1999.)
B1997 | Passenger-side side air bag module circuit short to body ground
B1998 | Passenger-side side air bag module circuit resistance high
B1999 | Passenger-side side air bag module circuit resistance low
B2226 | Crash zone sensor (internal circuit abnormal) | (See DTC B104D, B2226, B2227, B2855.)
B2227 | Crash zone sensor (communication error)
B2228 | Driver-side air bag module (inflator No.2) circuit short to body ground | (See DTC B1058, B2228, B2230, B2232, B2234.)
B2229 | Passenger-side air bag module (inflator No.2) circuit short to body ground | (See DTC B1059, B2229, B2231, B2233, B2235.)
B2230 | Driver-side air bag module (inflator No.2) circuit short to power supply | (See DTC B1058, B2228, B2230, B2232, B2234.)
B2231 | Passenger-side air bag module (inflator No.2) circuit short to power supply | (See DTC B1059, B2229, B2231, B2233, B2235.)
B2232 | Driver-side air bag module (inflator No.2) circuit resistance high | (See DTC B1058, B2228, B2230, B2232, B2234.)
B2233 | Passenger-side air bag module (inflator No.2) circuit resistance high | (See DTC B1059, B2229, B2231, B2233, B2235.)
B2234 | Driver-side air bag module (inflator No.2) circuit resistance low | (See DTC B1058, B2228, B2230, B2232, B2234.)
B2235 | Passenger-side air bag module (inflator No.2) circuit resistance low | (See DTC B1059, B2229, B2231, B2233, B2235.)
B2432 | Driver-side front buckle switch circuit open | (See DTC B1053, B2432, B2433, B2434, B2435.)
B2433 | Driver-side front buckle switch circuit open or short to power supply
B2434 | Driver-side front buckle switch circuit short to body ground
B2435 | Driver-side front buckle switch circuit resistance not within specification
B2477 | Configuration error | (See DTC B2477.)
B2773 | Driver-side curtain air bag module circuit resistance low | (See DTC B1046, B2773, B2774, B2775, B2776.)
B2774 | Driver-side curtain air bag module circuit resistance high
B2775 | Driver-side curtain air bag module circuit short to body ground
B2776 | Driver-side curtain air bag module circuit short to power supply
B2777 | Passenger-side curtain air bag module circuit resistance low | (See DTC B1056, B2777, B2778, B2779, B2780.)
B2778 | Passenger-side curtain air bag module circuit resistance high
B2779 | Passenger-side curtain air bag module circuit short to body ground
B2780 | Passenger-side curtain air bag module circuit short to power supply
B2855 | Crash zone sensor circuit short | (See DTC B104D, B2226, B2227, B2855.)
B2856 | Crash zone sensor ID mismatch | (See DTC B2856, B2886, B2887.)
B2886 | Passenger-side side air bag sensor ID mismatch
B2887 | Driver-side side air bag sensor ID mismatch
U2017 | Driver-side side air bag sensor (communication error) | (See DTC B104B, B104E, B1051, U2017.)
U2018 | Passenger-side side air bag sensor (communication error) | (See DTC B104C, B104F, B1050, U2018.)