VARIABLE INTAKE-AIR SHUTTER VALVE ACTUATOR INSPECTION [Z6]

#
VARIABLE INTAKE-AIR SHUTTER VALVE ACTUATOR INSPECTION [Z6]

B3E011320130W02

## Operation Inspection

1. Disconnect the negative battery cable.

2. Remove the variable intake-air shutter valve actuator.

3. Connect the battery positive voltage to terminal A or B, and verify that the gear moves.

  • If there is no malfunction, carry out the "Circuit Open/Short Inspection".
  • If there is any malfunction, replace the variable intake-air shutter valve actuator.

Terminal | Gear rotation direction
--- | ---
A | B
B+ | GND | Counterclockwise
GND | B+ | Clockwise

## Circuit Open/Short Inspection

1. Inspect the following wiring harnesses for an open or short circuit. (Continuity check)

### Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the wiring harness.
  - Variable intake-air shutter valve actuator terminal A and PCM terminal 2AO
  - Variable intake-air shutter valve actuator terminal B and PCM terminal 2AS

### Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the wiring harness.
  - Variable intake-air shutter valve actuator terminal A and power supply
  - Variable intake-air shutter valve actuator terminal A and body GND
  - Variable intake-air shutter valve actuator terminal B and power supply
  - Variable intake-air shutter valve actuator terminal B and body GND