BRAKE PEDAL INSPECTION

#
BRAKE PEDAL INSPECTION

B3E041143300W03

## Pedal Height Inspection

1. Measure the distance from the center of the upper surface of the pedal pad to the floor covering and verify that it is as specified.

  • If not within the specification, replace the brake pedal.

  Pedal height (reference value)
  136.4 mm {5.37 in}

## Pedal Play Inspection

1. Pump the pedal several times to release the vacuum in the power brake unit.

2. Gently depress the pedal by hand and measure the pedal play.

  • If not within the specification, inspect the wear of the joint pin. Replace it if there is any malfunction.

  Standard pedal play
  4.0-8.4 mm {0.16-0.33 in}

  Note

  • If there is no malfunction in the joint pin, there is a possibility that the power brake unit has some malfunction. Verify that there are no malfunctions, and replace it if necessary.

## Pedal-to-floor Clearance Inspection

1. Start the engine and depress the brake pedal with a force of 147 N {15.0 kgf, 33.0 lbf}.

2. Measure the distance from the center of the upper surface of the pedal pad to the floor covering and verify that it is as specified.

  • If it is less than the specification, inspect for air in the brake line.

  Standard pedal-to-floor clearance
  89.8 mm {3.54 in} or more