WINDSHIELD WASHER HOSE REMOVAL/INSTALLATION

#
WINDSHIELD WASHER HOSE REMOVAL/INSTALLATION

B3E091967460W01

1. Remove the bonnet insulator. (See BONNET REMOVAL/INSTALLATION.)

2. Slightly bend back the mudguard (RH).

3. Disconnect joint pipe A.

4. Remove windshield washer hose A from clips A.

5. Remove clips B.

6. Disconnect windshield washer hose B from the washer nozzle.

7. Disconnect windshield washer hose C from the washer nozzle.

8. Disconnect joint pipe B, then remove windshield washer hose A, B and C.

9. Install in the reverse order of removal.