REAR DOOR REMOVAL/INSTALLATION

#
REAR DOOR REMOVAL/INSTALLATION

B3E091158010W03

1. Disconnect the negative battery cable.

2. To remove the checker, remove the following parts:

  (1) Regulator handle (vehicles with manual window system) (See REGULATOR HANDLE REMOVAL.) (See REGULATOR HANDLE INSTALLATION.)
  (2) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)
  (3) Rear door speaker (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

3. To remove the hinges, remove the following parts:

  (1) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (2) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Adjust the rear door. (See DOOR ADJUSTMENT.)

.

1 | Connector
2 | Bolt A
3 | Bolt B
4 | Rear door
5 | Bolt C
6 | Checker
7 | Nut
8 | Bolt D
9 | Rear door hinge