HEADLIGHT CLEANER HOSE REMOVAL/INSTALLATION

#
HEADLIGHT CLEANER HOSE REMOVAL/INSTALLATION

B3E091966122W11

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Disconnect the headlight cleaner hose A from the joint pipe.

4. Disconnect the headlight cleaner hose B from the headlight cleaner actuator.

5. Disconnect the headlight cleaner hose C from the headlight cleaner actuator.

6. Remove the headlight cleaner hose C from the clips.

7. Disconnect the joint pipe, then remove the headlight cleaner hose B and C.

8. Install in the reverse order of removal.