DTC TABLE [AUDIO SYSTEM]

#
DTC TABLE [AUDIO SYSTEM]

B3E090266900W04

Screen display | System malfunction location
--- | ---
DTC (When starting on-board diagnostic test function) | Error message (When error is found)
09: Er22 | - | Base unit (peripheral circuit for tuner)
09: Er20 | - | Power supply circuit to base unit
00: Er10 | - | Cassette deck communication circuit system
03: Er10 | - | CD player communication circuit system
05: Er10 | - | CD changer (external) communication circuit system
06: Er10 | - | CD changer (upper module) communication circuit system
07: Er10 | - | MD player communication circuit system
03: Er01 | - | CD player system
03: Er02 | CHECK CD | CD player system
03: Er07 | CHECK CD | CD player system
00: Er01 | - | Cassette deck system
00: Er03 | - | Cassette deck system
00: Er04 | CHECK TAPE | Cassette tape system
05: Er01 | - | CD changer (external) system
05: Er07 | CHECK CD | CD changer (external) system
06: Er01 | - | CD changer (upper module) system
06: Er02 | CHECK CD | CD changer (upper module) system
06: Er07 | CHECK CD | CD changer (upper module) system
07: Er01 | - | MD player system
07: Er02 | CHECK MD | MD player system
07: Er07 | CHECK MD | MD player system
07: Er08 | CHECK MD | MD system
10: Er01 | - | MP3 applicable CD player system
10: Er02 | CHECK CD | MP3 applicable CD player system
no Er | - | No DTCs stored