DISCHARGE HEADLIGHT CONTROL MODULE REMOVAL/INSTALLATION

#
DISCHARGE HEADLIGHT CONTROL MODULE REMOVAL/INSTALLATION

B3E091851030W03

  Warning

  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the discharge headlight service warnings. (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Remove screws.

5. Disconnect the connector.

6. Remove the discharge headlight control module.

7. Install in the reverse order of removal.