DTC TABLE [LF]

#
DTC TABLE [LF]

B3E010200102W11
×: Applicable
-: Not applicable

DTC No. | Condition | MIL | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | ---
P0031 | Front HO2S heater circuit low input | ON | 2 | HO2S heater | × | (See DTC P0031 [LF])
P0032 | Front HO2S heater circuit high input | ON | 2 | HO2S heater | × | (See DTC P0032 [LF])
P0037 | Rear HO2S heater circuit low input | ON | 2 | HO2S heater | × | (See DTC P0037 [LF])
P0038 | Rear HO2S heater circuit high input | ON | 2 | HO2S heater | × | (See DTC P0038 [LF])
P0101 | MAF sensor circuit range/performance problem | ON | 2 | CCM | × | (See DTC P0101 [LF])
P0102 | MAF sensor circuit low input | ON | 1 | CCM | × | (See DTC P0102 [LF])
P0103 | MAF sensor circuit high input | ON | 1 | CCM | × | (See DTC P0103 [LF])
P0107 | MAP sensor circuit low input | ON | 1 | CCM | × | (See DTC P0107 [LF])
P0108 | MAP sensor circuit high input | ON | 1 | CCM | × | (See DTC P0108 [LF])
P0111 | IAT sensor circuit range/performance problem | ON | 2 | CCM | × | (See DTC P0111 [LF])
P0112 | IAT sensor circuit low input | ON | 1 | CCM | × | (See DTC P0112 [LF])
P0113 | IAT sensor circuit high input | ON | 1 | CCM | × | (See DTC P0113 [LF])
P0117 | ECT sensor circuit low input | ON | 1 | CCM | × | (See DTC P0117 [LF])
P0118 | ECT sensor circuit high input | ON | 1 | CCM | × | (See DTC P0118 [LF])
P0121 | TP sensor stuck closed | ON | 2 | CCM | × | (See DTC P0121 [LF])
P0122 | TP sensor circuit low input | ON | 1 | CCM | × | (See DTC P0122 [LF])
P0123 | TP sensor circuit high input | ON | 1 | CCM | × | (See DTC P0123 [LF])
P0125 | Excessive time to enter closed loop fuel control | ON | 2 | CCM | × | (See DTC P0125 [LF])
P0132 | Front HO2S circuit high input | ON | 2 | HO2S | × | (See DTC P0132 [LF])
P0133 | Front HO2S circuit problem | ON | 2 | HO2S | × | (See DTC P0133 [LF])
P0134 | Front HO2S no activity detected | ON | 2 | HO2S | × | (See DTC P0134 [LF])
P0138 | Rear HO2S circuit high input | ON | 2 | HO2S | × | (See DTC P0138 [LF])
P0140 | Rear HO2S no activity detected | ON | 2 | HO2S | × | (See DTC P0140 [LF])
P0300 | Random misfire detected | Flash/ON | 1 or 2 | Misfire | × | (See DTC P0300 [LF])
P0301 | Cylinder No.1 misfire detected | Flash/ON | 1 or 2 | Misfire | × | (See DTC P0301, P0302, P0303, P0304 [LF])
P0302 | Cylinder No.2 misfire detected | Flash/ON | 1 or 2 | Misfire | ×
P0303 | Cylinder No.3 misfire detected | Flash/ON | 1 or 2 | Misfire | ×
P0304 | Cylinder No.4 misfire detected | Flash/ON | 1 or 2 | Misfire | ×
P0327 | KS circuit low input | ON | 1 | CCM | × | (See DTC P0327 [LF])
P0328 | KS circuit high input | ON | 1 | CCM | × | (See DTC P0328 [LF])
P0335 | CKP sensor circuit problem | ON | 1 | CCM | × | (See DTC P0335 [LF])
P0340 | CMP sensor circuit problem | ON | 1 | CCM | × | (See DTC P0340 [LF])
P0403 | EGR valve (stepper motor) circuit problem | ON | 2 | CCM | × | (See DTC P0403 [LF])
P0420 | Catalyst system efficiency below threshold | ON | 2 | Catalyst | × | (See DTC P0420 [LF])
P0443 | Purge solenoid valve circuit problem | ON | 2 | CCM | × | (See DTC P0443 [LF])
P0480 | Cooling fan control circuit problem | OFF | 1 | Other | × | (See DTC P0480 [LF])
P0500 | VSS circuit problem | ON | 2 | CCM | × | (See DTC P0500 [LF])
P0505 | IAC system problem | OFF | - | Other | - | (See DTC P0505 [LF])
P0506 | Idle control system RPM lower than expected | ON | 2 | CCM | × | (See DTC P0506 [LF])
P0507 | Idle control system RPM higher than expected | ON | 2 | CCM | × | (See DTC P0507 [LF])
P0511 | IAC valve circuit problem | ON | 1 | CCM | × | (See DTC P0511 [LF])
P0602 | PCM programming error | ON | 1 | CCM | × | (See DTC P0602 [LF])
P0610 | PCM vehicle options error | ON | 1 | CCM | × | (See DTC P0610 [LF])
P0661 | Variable intake-air solenoid valve circuit low input | OFF | 1 | Other | × | (See DTC P0661 [LF])
P0662 | Variable intake-air solenoid valve circuit high input | OFF | 1 | Other | × | (See DTC P0662 [LF])
P0703 | Brake switch input circuit problem | ON | 2 | CCM | × | (See DTC P0703 [LF])
P0704 | CPP switch input circuit problem | ON | 2 | CCM | × | (See DTC P0704 [LF])
P0706 | Transaxle range (TR) switch circuit range/performance | (See DTC TABLE [FN4A-EL].)
P0707 | Transaxle range (TR) switch circuit low input | (See DTC TABLE [FN4A-EL].)
P0708 | Transaxle range (TR) switch circuit high input | (See DTC TABLE [FN4A-EL].)
P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (stuck) | (See DTC TABLE [FN4A-EL].)
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short to ground) | (See DTC TABLE [FN4A-EL].)
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | (See DTC TABLE [FN4A-EL].)
P0715 | Input/turbine speed sensor circuit malfunction | (See DTC TABLE [FN4A-EL].)
P0731 | Gear 1 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0732 | Gear 2 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0733 | Gear 3 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0734 | Gear 4 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0741 | Torque converter clutch (TCC) (stuck off) | (See DTC TABLE [FN4A-EL].)
P0742 | Torque converter clutch (TCC) (stuck on) | (See DTC TABLE [FN4A-EL].)
P0745 | Pressure control solenoid malfunction | (See DTC TABLE [FN4A-EL].)
P0751 | Shift solenoid A stuck off | (See DTC TABLE [FN4A-EL].)
P0752 | Shift solenoid A stuck on | (See DTC TABLE [FN4A-EL].)
P0753 | Shift solenoid A malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0756 | Shift solenoid B stuck off | (See DTC TABLE [FN4A-EL].)
P0757 | Shift solenoid B stuck on | (See DTC TABLE [FN4A-EL].)
P0758 | Shift solenoid B malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0761 | Shift solenoid C stuck off | (See DTC TABLE [FN4A-EL].)
P0762 | Shift solenoid C stuck on | (See DTC TABLE [FN4A-EL].)
P0763 | Shift solenoid C malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0766 | Shift solenoid D stuck off | (See DTC TABLE [FN4A-EL].)
P0767 | Shift solenoid D stuck on | (See DTC TABLE [FN4A-EL].)
P0768 | Shift solenoid D malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0771 | Shift solenoid E stuck off | (See DTC TABLE [FN4A-EL].)
P0772 | Shift solenoid E stuck on | (See DTC TABLE [FN4A-EL].)
P0773 | Shift solenoid E malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0850 | Neutral switch input circuit problem | ON | 2 | CCM | × | (See DTC P0850 [LF])
P0894 | Forward clutch torque transmission | (See DTC TABLE [FN4A-EL].)
P1260 | Immobilizer system problem | OFF | 1 | Other | × | (See DTC P1260 [LF])
P2006 | Variable tumble shutter valve stuck closed | ON | 2 | CCM | × | (See DTC P2006 [LF])
P2009 | Variable tumble solenoid valve circuit low input | ON | 2 | CCM | × | (See DTC P2009 [LF])
P2010 | Variable tumble solenoid valve circuit high input | ON | 2 | CCM | × | (See DTC P2010 [LF])
P2096 | Target A/F feedback system too lean | ON | 2 | Fuel system | × | (See DTC P2096 [LF])
P2097 | Target A/F feedback system too rich | ON | 2 | Fuel system | × | (See DTC P2097 [LF])
P2177 | Fuel system too lean at off idle | ON | 2 | Fuel system | × | (See DTC P2177 [LF])
P2178 | Fuel system too rich at off idle | ON | 2 | Fuel system | × | (See DTC P2178 [LF])
P2187 | Fuel system too lean at idle | ON | 2 | Fuel system | × | (See DTC P2187 [LF])
P2188 | Fuel system too rich at idle | ON | 2 | Fuel system | × | (See DTC P2188 [LF])
P2195 | Front HO2S signal stuck lean | ON | 2 | HO2S | × | (See DTC P2195 [LF])
P2196 | Front HO2S signal stuck rich | ON | 2 | HO2S | × | (See DTC P2196 [LF])
P2228 | BARO sensor circuit low input | ON | 1 | CCM | × | (See DTC P2228 [LF])
P2229 | BARO sensor circuit high input | ON | 1 | CCM | × | (See DTC P2229 [LF])
P2502 | Charging system voltage problem | OFF | 1 | Other | × | (See DTC P2502 [LF])
P2503 | Charging system voltage low | OFF | 1 | Other | × | (See DTC P2503 [LF])
P2504 | Charging system voltage high | OFF | 1 | Other | × | (See DTC P2504 [LF])
P2507 | PCM B+ voltage low | ON | 1 | CCM | × | (See DTC P2507 [LF])
U0073 | CAN system communication error | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0121 | Communication error to ABS HU/CM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0155 | Communication error to instrument cluster | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])