DTC 07:ER01

#
DTC 07:ER01

B3E090266900W20

DTC 07:Er01 | MD player
DETECTION CONDITION | • MD player cannot implement insert and eject commands.
POSSIBLE CAUSE | • Defective MD (broken or foreign material stuck/attached) • MD player malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Can MD be ejected? | Yes | Go to the next step.
No | Replace the MD player.
2 | Verify the condition of the MD when the error occurs. Is the MD normal? | Yes | Go to the next step.
No | Repair (remove foreign material) or replace the MD, and go to the next step.
3 | Clear the DTC. Insert then eject a normal MD. Is DTC 07: Er01 displayed? | Yes | Replace the MD player.
No | DTC troubleshooting completed.