SOLENOID VALVE REMOVAL/INSTALLATION

#
SOLENOID VALVE REMOVAL/INSTALLATION

B3E051721280W02

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Disconnect the negative battery cable.

3. Remove the under cover.

4. Remove the control valve body. (See CONTROL VALVE BODY REMOVAL.)

5. Remove the solenoid valve(s).

6. Apply ATF to a new O-ring and install it on the solenoid valve.

7. Install the solenoid valve in the control valve body.

  Tightening torque
  7.8-10.8 N·m
  {80-110 kgf·cm, 69.5-95.4 in·lbf}

8. Install the control valve body. (See CONTROL VALVE BODY REMOVAL.)

9. Install the under cover.

10. Connect the negative battery cable.

11. Install the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

12. Add ATF and, with the engine idling, inspect the ATF level and inspect for leakage. (See Automatic Transaxle Fluid (ATF) Level Inspection.)

13. Perform the mechanical system test. (See MECHANICAL SYSTEM TEST.)

14. Perform the road test. (See ROAD TEST.)