CLIMATE CONTROL UNIT INSTALLATION [MANUAL AIR CONDITIONER]

#
CLIMATE CONTROL UNIT INSTALLATION [MANUAL AIR CONDITIONER]

B3E074061190W03

1. Pass each wire through the following routes and connect to A/C unit.

2. Connect the climate control unit connectors.

3. Adjust the climate control unit wires. (See CLIMATE CONTROL UNIT WIRE ADJUSTMENT.)

4. Install the following parts:

  (1) PJB and PJB bracket. (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)
  (2) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  (3) Decoration panel (SeeDECORATION PANEL REMOVAL/INSTALLATION.)
  (4) Front side trim (RH) (SeeFRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (5) Front scuff plate (RH) (SeeFRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (6) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)
  (7) Front side trim (SeeFRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (8) Front scuff plate (SeeFRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (9) Detach the bonnet release lever from the lower panel. (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [L.H.D.].) (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION [R.H.D.].)
  (10) Ashtray panel (See CONSOLE REMOVAL/INSTALLATION.)
  (11) Climate control unit
  (12) Center panel module (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

5. Connect the negative battery cable.