NEUTRAL SWITCH INSPECTION [LF]

#
NEUTRAL SWITCH INSPECTION [LF]

B3E014017640W03

  Note

  • Before performing the following inspection, make sure to follow the procedure as indicated in the troubleshooting flowchart.

## Continuity Inspection

1. Remove the neutral switch. (See NEUTRAL SWITCH REMOVAL/INSTALLATION [G35M-R].)

2. Verify that the continuity between neutral switch terminals A and B is as indicated in the table.

  • If it can be verified, perform the "Circuit Open/Short Inspection".
  • If it cannot be verified, replace the neutral switch.

Measured condition | Continuity
--- | ---
Rod pushed | Continuity detected
Except above | No continuity

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [LF].)

2. Inspect the following harness for open or short. (Continuity check)

### Open circuit

  • Neutral switch terminal A and PCM terminal 1S
  • Neutral switch terminal B and body GND

### Short circuit

  • Neutral switch terminal B and body GND