GPS ANTENNA REMOVAL/INSTALLATION

#
GPS ANTENNA REMOVAL/INSTALLATION

B3E092066936W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front scuff plate (Passenger's side) (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (2) Front side trim (Passenger's side) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (3) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)
  (4) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  (5) Car-navigation unit (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)
  (6) Passenger junction box (PJB) (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | GPS antenna

4. Install in the reverse order of removal.