TRANSMITTER BATTERY REPLACEMENT

#
TRANSMITTER BATTERY REPLACEMENT

B3E091467543W01

1. Insert a small screwdriver into the slot and gently pry open the transmitter.

2. Press the portion of the battery indicated by A and remove the battery.

3. Install a new battery (CR2025) into the front portion of the holder with the positive pole (+) facing up. Press on the B portion of the battery to set the battery.

4. Align the front and back covers and snap the transmitter shut.

  Battery specification
  Lithium CR2025 × 1

  Note

  • The batteries will last about 2 years when used 10 times a day.