WATER PUMP REMOVAL/INSTALLATION [ZJ, Z6]

#
WATER PUMP REMOVAL/INSTALLATION [ZJ, Z6]

B3E011215010W01

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].)

2. Disconnect the negative battery cable.

3. Remove the under cover and splash shield as a single unit.

4. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT.)

5. Set the coolant reserve tank out of the way.

6. Remove the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, Z6].)

7. Set the power steering fluid tank out of the way.

8. Remove the generator. (See GENERATOR REMOVAL/INSTALLATION [ZJ, Z6].)

9. Remove in the order indicated in the table.

.

1 | Water pump component
2 | O-ring

10. Install in the reverse order of removal.

11. Add engine coolant. (See ENGINE COOLANT REPLACEMENT.)

12. Inspect for engine coolant leakage. (See ENGINE COOLANT LEAKAGE INSPECTION.)