PARKING BRAKE LEVER INSPECTION

#
PARKING BRAKE LEVER INSPECTION

B3E041244300W04

## Stroke Inspection

1. Pump the brake pedal a few times.

2. Pull the parking brake lever two to three times.

3. Inspect the parking brake stroke by slowly pulling at point A 50 mm {1.97 in} from the end of the parking brake lever with a force of 98 N {10 kgf, 22 lbf} and counting the number of notches (clicking sound).

  • If not within the specification, adjust the parking brake lever.

  Standard
  3-6 notches