SUNROOF MOTOR REMOVAL/INSTALLATION

#
SUNROOF MOTOR REMOVAL/INSTALLATION

B3E091569873W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Console (4SD) (See CONSOLE REMOVAL/INSTALLATION.)
  (2) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (3) Upper anchor of the front seat belt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)
  (4) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (5) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (6) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)
  (7) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)
  (8) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (9) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (10) Trunk side upper trim (5HB) (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION.)
  (11) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)
  (12) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (13) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (14) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (15) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)
  (16) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

3. Disconnect the sunroof motor connector.

4. Remove the screws, then remove the sunroof motor.

5. Install in the reverse order of removal.

  Note

  • If the glass panel or the sunroof motor is moved with the sunroof motor removed, initial position setting of the sunroof motor will be required. Perform initial position setting referring to the Sunroof Motor Assembly Note. (See Sunroof Motor Assembly Note.)