VARIABLE TUMBLE SOLENOID VALVE INSPECTION [LF]

#
VARIABLE TUMBLE SOLENOID VALVE INSPECTION [LF]

B3E011318740W02

1. Remove the variable tumble solenoid valve. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [LF].)

2. Inspect airflow between the ports under the following conditions.

  • If not as specified, replace the variable tumble solenoid valve.
  • If as specified, carry out the "Circuit Open/Short Inspection".

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [LF].)

2. Inspect the following wiring harness for open or short (continuity check).

### Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the wiring harness.
  - Variable tumble solenoid valve terminal B and PCM terminal 2AI
  - Variable tumble solenoid valve terminal A and main relay terminal A

### Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the wiring harness.
  - Variable tumble solenoid valve terminal A and body GND
  - Variable tumble solenoid valve terminal B and power supply